|  |  |  |
| --- | --- | --- |
|  | **Wall-mounted version** | **Hand-held version** |
| **Kích thước** (length x width x height) | 265x185x180mm (including protruding parts) | 110x130x68mm (including protruding parts) |
| **Weight** | ~ 300g | ~ 200g |
| **Input voltage** | DC 5V | - |
| **Chargable battery** | Optional | Default |
| **Charging port** | 5V Micro USB | |
| **Battery capacity** | 2000mAh | |
| **Main board** | ATmega328P (Arduino board) + ESP32 | ATmega328P  (Arduino board) |
| **Proximity sensor** | E18-D50NK | - |
| **Infrared thermometer** | Melexis MLX90614 non-contact | |
| **Display screen** | OLED 1.3inch | |
| **Cord for other screen** | - | I2C (4pin) |
| **Connection** | Wifi, Bluetooth | - |